**Pasi pentru creare etichete patch panel cu**

**aparat de etichetare industrial**

**Dymo Rhino 6000+**

****

Modul de etichetare patch panel va permite sa etichetati un rand de porturi.

Doar selectati distanta dintre porturi, introduceti textul si printati.

Rezultatul consta intr-o eticheta durabila cu spatii egale si informatii pentru fiecare port in parte.

**Pentru a crea o eticheta pentru patch panel:**

 1. Apasati **PPANEL**;

 2. Selectati **Port distance** (Distanta dintre porturi sau celule);

 3. Introduceti distanta dintre fiecare port si apasati **OK**;

 4. Selectati **# of ports** (nr porturi sau celule);

 5. Introduceti numarul de porturi si apasati **OK**;

 6. Selectati **Done (ESC)** pentru a crea o eticheta.

EN

**Steps for creating patch panel labels with**

**industrial labeling machine**

**Dymo Rhino 6000+**

****

The patch panel labeling mode allows you to label a row of ports.

Just select the distance between the ports, enter the text and print.

The result is a durable label with equal spaces and information for each port.

**To create a patch panel label:**

 1. Click **PPANEL**;

 2. Select Port distance;

 3. Enter the distance between each port and press **OK**;

 4. Select **# of ports** (no ports or cells);

 5. Enter the number of ports and press **OK**;

 6. Select **Done (ESC)** to create a label.